**Information on product discontinuation**

**Dear Customers,**

**Herewith we would like to inform you about changes in our product range.**

**All article numbers of the product SKINDICHT® SE as well as the multi-entries of the product SKINDICHT® SE-M will be discontinued.**

**The items can be ordered until the remaining quantities of the basic housings are sold out.**

**The PG single entries of the product SKINDICHT® SE can be replaced by the metric single entries of the product SKINDICHT® SE-M. The housing dimensions and technical characteristics of the articles listed below are comparable. The difference is now the metric connection thread for the used cable glands. For every LAPP PG cable gland, you will find a metric LAPP counterpart. We are happy to advise you on this.**

**While discontinuing the PG variants, the product SKINDICHT® SE-M will be optimized. The housings of the remaining article numbers will be lighter, and the surface coating will be changed from hammer finish lacquered to nickel-plated. Nickel-plated surfaces are standard at LAPP, and it promises better corrosion protection as well as a modern design.**

**The hammerstone variant will be delivered until the available stock of the basic housings is sold out. Afterwards, the article numbers will be switched to the nickel-plated variant.**

[https://www.lapp.com/en/de/skindicht-se-m](https://www.lapp.com/en/de/skindicht-se-m/p/52108000)

[https://www.lapp.com/en/de/skindicht-se-m-without-e-d](https://www.lapp.com/en/de/skindicht-se-m-without-e-d/p/52108001)

[https://www.lapp.com/en/de/skindicht-se-m-220/320](https://www.lapp.com/en/de/skindicht-se-m-220/320/p/52108040)

[https://www.lapp.com/en/de/skindicht-se-m-220/320-without-e-d](https://www.lapp.com/en/de/skindicht-se-m-220/320-without-e-d/p/52108041)

[https://www.lapp.com/en/de/skindicht-se](https://www.lapp.com/en/de/skindicht-se/p/52004130)

[https://www.lapp.com/en/de/skindicht-se-without-e-d](https://www.lapp.com/en/de/skindicht-se-without-e-d/p/52024090)

**Article Overview Product Discontinuation:**

|  |  |  |  |
| --- | --- | --- | --- |
| **Discontinued product** | | **Alternative product** | |
| **Article number** | **Material description** | **Article number** | **Material description** |
| 52004130 | SKINDICHT® SE PG 16 | 52108000 | SKINDICHT® SE-M 20X1,5 |
| 52024090 | SKINDICHT® SE PG 16 O. E+D | 52108001 | SKINDICHT® SE-M 20X1,5 O. E+D |
| 52004140 | SKINDICHT® SE PG 21 | 52108010 | SKINDICHT® SE-M 25X1,5 |
| 52024100 | SKINDICHT® SE PG 21 O. E+D | 52108011 | SKINDICHT® SE-M 25X1,5 O. E+D |
| 52005430 | SKINDICHT® SE PG 29 | 52108020 | SKINDICHT® SE-M 32X1,5 |
| 52024110 | SKINDICHT® SE PG 29 O. E+D | 52108021 | SKINDICHT® SE-M 32X1,5 O. E+D |
| 52004150 | SKINDICHT SE PG 36 | **X** | **X** |
| 52024120 | SKINDICHT SE PG 36 O. E+D | **X** | **X** |
| 52005290 | SKINDICHT SE PG 216 | **X** | **X** |
| 52024121 | SKINDICHT SE PG 216 o. E+D | **X** | **X** |
| 52108040 | SKINDICHT SE-M 220 | **X** | **X** |
| 52108041 | SKINDICHT SE-M 220 O. E+D | **X** | **X** |
| 52005300 | SKINDICHT SE PG 316 | **X** | **X** |
| 52024123 | SKINDICHT SE PG 316 o. E+D | **X** | **X** |
| 52108050 | SKINDICHT SE-M 320 | **X** | **X** |
| 52108051 | SKINDICHT SE-M 320 O. E+D | **X** | **X** |

**All information can also be found on our website in the** [**product notifications**](https://www.lapp.com/de/de/produkte/produktbenachrichtigungen/e/000302) **section:**

<https://www.lapp.com/en/de/products/product-notifications/e/090901>

**We will be happy to send you more detailed information and advise you personally. Please get in touch with your sales representative or contact person at internal** **sales.**

**We are confident that we will continue to present you with an appealing range of products and will be happy to answer any questions you may have.**

**With kind regards**

**U.I. Lapp GmbH**